EIO Tube

40 dB Coupler

Switch

HP Power Meter

EIP Frequency Meter

10 dB Coupler

Microwave Dump

Microwave Horn

Carbon

F-band Waveguide (90-140 GHz)

D-band Waveguide (110-170 GHz)

V-band Oversized Waveguide (50-75 GHz)

Transition to D-band Transition to V-band

Transition to Circular

Waveguide

Top of Insert

Deuteron Cup

Proton Cup

Empty Cup

Residual Proton Coil

Proton Coil

Deuteron/ N15 in ND3 Coil

N15 in NH3 Coil

Dummy Coils

The Target Cup and Coil Configuration